Afbeelding met ketting

Automatisch gegenereerde beschrijving

**\*AVAILABLE WITH 3 DIFFERENT CHAIN LENGTHS**

**IMPA Number: 615006**

**Product code:   
  
8589 = 3 M  
10623 = 6 M  
10624 = 9 M**

● GBO heat treated alloy load chain.

● Forged alloy Steel Hooks. Industrial rated hooks rotate 360 degrees for easy rigging.


● Sealed roller bearings. Greatly improving performance and serve life of the product.

● Load tested to 150% of capacity with test certificate.

**Product specs:**

|  |  |
| --- | --- |
| TYPE | 4025 |
| Max capacity | 500 Kg |
| Tested capacity | 750 KG |
| Max lifting height | See next page |
| Material | Steel alloy |
| Chain material | Steel alloy |
| Type | Manual chain hoist |
| Max effort required to lift | 300 N |
| Approvals | CE approved |





Afbeelding met rood

Automatisch gegenereerde beschrijving

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CODE** | **WLL (T)** | **Lift(m)** | **Load Chain** | | **Dimensions (mm)** | | | | **N.W.(kg)** | **G.W.(kg)** | **Packed size (cm)** |
| **Falls** | **Size** | **A** | **B** | **D** | **H** |
| **8589** | 0.5 | 3 | 1 | 6X18 | 137 | 137.5 | 35 | 270 | 8.7 | 10.1 | 24 x 20 x 20 |
| **10623** | 0.5 | 6 | 1 | 6X18 | 137 | 137.5 | 35 | 270 | 13.3 | 14.7 | 24 x 20 x 20 |
| **10624** | 0.5 | 9 | 1 | 6X18 | 137 | 137.5 | 35 | 270 | 18.2 | 19.7 | 27 x 21 x 21 |